**Annex 1– Technical specification of the subject matter**

Contracting Authority requires delivery of new goods in accordance with the minimum requirements specified below.

**Device for non-destructive test and verification the vehicle identification number**

Abstract:

The measuring device must be capable of non-destructive method verify the authenticity of identifiers (VIN, chassis number). The device must be able to detect unauthorized manipulation with the VIN characters and near the VIN on the basis of changes the structure of the material.

Required properties:

* device must be able to measure property sheet metal (microstructure)
* device must be able to detect changes in of plasticity vehicle identification number
* device must be able to detect changes in the structure and condition of material around vehicle's identifiers
* device must be mobile
* device must be able to connection to PC
* device must have the possibility mains power and its own battery
* device must have its own software for evaluating and archiving of measured data
* delivery devices including accessories and software for immediate use